/*========== START Qt6 migration:
**
void tst_MainWindow::test_focusOrder()
Test: // qApplication::setActiveWindow(mainWindow);
I had to replace previews line.

**
void DataBase::compress()
qsqldatabase::exec is deprecated

**
void eLogQrzLog::parseXMLAnswer(QXmlStreamReader &xml)
{ // Next line was commented out as it returns q QStringView instead of a QString
    //showDebugLog (Q_FUNC_INFO, QString("Start: " + xml.text()));

=============== END of Qt6 migration



BUG: KLog needs to update the Entity DB is shown on every start

KLog should update ALWAYS when receiving from LoTW the QSL_LOTW_rcvd or add the QSO if not in local log.

Review the process after Setup


TODO: Integrate HAMQTH https://www.hamqth.com/developers.php
TODO:- New feature: Regional Award support: #include "setuppages/setuppagesubdivisions.h"

TODO: Stat More frequently worked calls: "select log.call, count(log.call) from log group by log.call ORDER BY count(log.call) DESC"
TODO: Stat Number of different callsigns
TODO: Find "duplicated" QSOs QUERY=> SELECT call, bandid, modeid, substr(qso_date, 1, 15), COUNT(*) c FROM log GROUP BY call, bandid, modeid, substr(qso_date, 1, 15) HAVING c>1
TODO: Find duplicate queries:
select call, qso_date from log where datetime('2007-07-22 09:45:00', '-5 minutes')< datetime(qso_date) AND datetime('2007-07-22 09:49:00', '+5 minutes') > datetime(qso_date)
select call, qso_date, bandid, modeid, COUNT(*) c from log  where datetime('2010-10-31 19:20:00', '-5 minutes')< datetime(qso_date) AND datetime('2010-10-31 19:20:00', '+5 minutes') > datetime(qso_date) group by call having c>1


RC-BUGS:


TODO: Check if dxccStatusWidget in logwindow is useful and remove it if not.
NONE

TODO: New feature: KLog can now control a rotator through PSTRotator.
TODO: UI: Added a DXCC summary obtained from the Tools menu.

TBD - 0.9.8
Hamlib: COMports in Windows must follow the format: \\.\com14 for ports highet than 9 but it works also for lower so ALL should be managed that way.

For next release:
TODO: - Some warnings removed from compilation time.
TODO: - The log can be now updated with a LoTW ADIF file import.
TODO: - Isolate the Awards tab and create a widget with it.
TODO: - ADD A TIP ON the DXCC tab stating Prefix, CQ, ITU & Bearing.
TODO: Rework the band & mode hash tables to optimize queries (not sql queries)
TODO: Rework the DXCC & WAZ hash table sto optimize queries (not SQL queries)

TODO: Import LOTW (MainWindow::slotADIFImport)
TODO: Remove the Querys from void SetupPageLogs::

TODO: Create a Widget with the WAZ status (copying the DXCC Status widget)

Working:
TODO: ADD A TIP ON the DXCC tab stating Prefix, CQ, ITU & Bearing


TODO: Check how to implement qInstallMessageHandler
SAT DB: https://db.satnogs.org/api/

This is a kind of roadmap for KLog development.
It is not fixed... new features may be prioritized or not added without any notice ;-)
Feel free to request any roadmap change if you have any suggestion.

TODO: To add the support to import/export the following ADIF fields that are already existing in DB
    AWARD_SUBMITTED
    AWARD_GRANTED
    DARC_DOK
    FISTS
    FISTS_CC
    GUEST_OP
    "hrdlog_qso_upload_date VARCHAR(10),"
    "hrdlog_qso_upload_status  VARCHAR(1),"
    "my_antenna VARCHAR,"
    "my_dxcc INTEGER, "
    "my_fists INTEGER, "
    "my_itu_zone INTEGER ,"
    "my_postal_code VARCHAR ,"
    "my_sota_ref VARCHAR, "
    "my_usaca_counties VARCHAR, "
    "my_vucc_grids VARCHAR, "
    "silent_key VARCHAR(1), "
    "region VARCHAR, "
    "qrzcom_qso_upload_date VARCHAR(10), "
    "qrzcom_qso_upload_status VARCHAR(1), "
    "skcc VARCHAR, "
    "sota_ref VARCHAR, "
    "uksmg INTEGER, "
    "usaca_counties VARCHAR, "
    "ve_prov VARCHAR, "
    "vucc_grids VARCHAR, "


TODO: Add a warning or periodically ADIF export so data is backup
TODO: Create a function to look for QSO without a DXCC and ask the user to confirm the DXCC.
TODO: Isolate the QSO input tab and create a widget with it.
TODO: Isolate the Main QRZ box and create a widget with it.
TODO: Isolate the Awards tab and create a widget with it.
TODO: Add an option to save the DXCluster data to a file (file based on name or so)

TODO: Think if it is possible to create a function in the Widgets(i.e. MainWindowInputQSL) to read the data and
        enter it in the DB automatically when the user clicks on "enter"
        It would help to "isolate" it and make it more "independant"

TODO: Review the color management in MainWindowInputOthers::setIOTA (and maybe others) (completewithPrevious of MainWindow)
TODO: Check if in mainwindow (read formUI and modify the eQSL/LOTW REC/SENT values are correct

TODO: If no QSL sent via or rec via are defined, KLog shows as direct? It should be bureau


TODO: Add a cheking to the list of bureaus and propose the bureau for QSL via when there is an existing one and propose direct when no bureau is existing.
      (http://www.iaru.org/qsl-bureaus.html)

TODO: Define band limits for CW/SSB/RTTY... so when a click on the cluster is done, the right mode is proposed.
TODO: Add in the setup/Band/mode a combobox showing all the active band/modes so the user can select the default band/mode from that list.

BUG: Potential bug
Double click on a QSO in the log on the Mode/Band... you can modifify the value. As it is a double click, the QSO goes to edit and ...
Check if:
  - Only selected modes can be shown there.
  - If double click on the log we only "quick modify" directly in the log, without editing.

BUG: (TNX JL3OXR)
The DB is not storing if the time is stored in UTC or local so that info is lost.
If a user changes the configuration from time to time, the user will loose the real time when the QSO was made.
Solution:
 - Consider the DB is only storing UTC QSO.
 - Read config from user (or simply ask) and convert all the DB to UTC if needed (only one time when new version is installed to upgrade the DB)
 Always:
 - When entering data from the UI, check the user config and store only UTC time.
 - TODO: Think how to show the data in the log or search box as data is stored in UTC and showed directly (specially log widget)
    - Solution: Maybe changing the header to UTC may solve this and provide the info to the user that UTC is being used for storage
        It may be weird for the user to see the log in UTC when working in local time... in the rest of the functions...


TODO: void DXCCStatusWidget::slotRefreshButtonClicked()//TODO: Define a way to show the status of the selected log or all the logs in the DB

BUG: Optimize the KLog start
BUG: If logbook.dat is not existing but klogrc it is, KLog does not start.

TODO: Add a tip on the DXCC Status showing some info: bearing, DXCC status (worked or not...)
TODO: Add a link or action on DXCCStatus items to doubleclick and search the QSOs that provide such status.

TODO: Show the flag of the worked QRZ on the top right,close to the Entity Name

TODO: Add the flags to the DXCluster
TODO: Click on an Entity name will select all the QSO of that Entity on the search box

Debian:

Time in UTC: (not to be fixed)
https://bugs.debian.org/cgi-bin/bugreport.cgi?bug=654325


BUG: Check the options that are marked in QSL when rightbutton.
i.e.: Is myQSL sent marked as requested when it should be the DX-QSL?

TODO GUI: To add the CQ/ITU box or make them editable
TODO: checkIfNewBandOrMode() is not being used. Code should be removed...

BUG:
Clublog:
void MainWindow::slotQRZReturnPressed()
_x = elogClublog->deleteQSO(clublogPrevQSO);
_x = elogClublog->sendQSO(dataProxy->getClubLogRealTimeFromId(modifyingQSOid))
It runs so fast and not serialized that at the end sometimes the QSO is deleted but not created afterwards


<CLUBLOG>
TODO: Add the possibility to the user to select from the setup a call to be used in clublog or use the one comming from the station callsign lineedit
TODO: In slotQsoUploadFinished, if QSO is not uploaded. mark it as not uploaded in the log

If qsoToEdit, nothing is modified and OK. (Clublog returns QSO DUPE)
Again qsoToEdit, nothing is modified and OK (Clublogs returns QSO DROPPED, and QSO is dropped!)

TODO: Check the values that clublog is returning to manage errors and show messages to the user
TODO: To add the possibility to upload a modified QSO to clublog.
TODO: If there is an error in password/username or whatever, disable clublog in KLog

TODO: Upload a logfile to clublog
// Ideas: https://code.google.com/p/datacod-qt-tools/source/browse/upcoder/uploader.h
// https://code.google.com/p/datacod-qt-tools/source/browse/upcoder/uploader.cpp

TODO: Define a maximum QSO upload rate to clublog to avoid excesive API usage.
</CLUBLOG>


KLog 0.9.4
TODO: Some Entities are not recognized by ARRL (I, IG9, IT9 are the same ARRL id entities but different ones). Maybe I should not be working
      with ARRLid or maybe I should detect special ones and "id+10000" so >10000 ids are special ones.


KLog 0.9.3
TODO: Support CQ WW SSB (Including Cabrillo Import/Export)
TODO: Support CQ WW CW (Including Cabrillo Import/Export)

KLog 0.9.4
TODO: Hamlib support (Linux).

KLog 0.9.5
TODO: Support CQ WPX SSB (Including Cabrillo Import/Export)
TODO: Support CQ WPX CW (Including Cabrillo Import/Export)

KLog 0.9.6
WORLDEDITOR Dialog
TODO: WorldEditor is not updated when the CTY.CSV file is updated
TODO: World Editor: Create a way to add an entity.
TODO: World Editor: Create a way to remove an entity.
TODO: World Editor: Create a way to edit an entity.

KLog 0.9.7
TODO: Integrate with www.clublog.org (http://www.clublog.org/docs/pages/viewpage.action?pageId=1638482)

KLog 0.9.8
TODO: Integrate with eqsl.cc
https://www.eqsl.cc/qslcard/ADIFContentSpecs.cfm

KLog 0.9.9
TODO: Server to log all the QSO in real time (through the network) from N1MM
        http://n1mm.hamdocs.com/tiki-index.php?page=UDP+Broadcasts&structure=N1MM+Logger+Documentation

KLog 0.9.10
TODO: Integrate with FLIGI real time logging (req by AA5VI)

KLog 0.9.11 - Cluster release
TODO: DXCluster: Add flags to the DXCluster widget
TODO: DXCluster: UI: Modify the DX-Cluster tab to show the data in a table?: DX de/Freq/DX/Comment/Time/Loc
TODO: DXCluster: Add the DXMarathon information to the spots
TODO: DXCLuster: Create a band map (including a "to-be-worked")
TODO: Working on the dxCluster: Tool to save the DXCluster in a file (for further analysis).

KLog 0.9.12
TODO: Add the awards functionality (to manage awa files, TPEA, WAS, ...)

KLog 0.9.13
TODO: Mobile interface. Create a mobile UI.

<BUGS>
TODO: Check if the data has been modified (only memory) and save the data!
TODO BUG: When modifying allow deleting data (as in KLog 0.5.8)
DONE BUG: Worked DXCC and WAZ are not updated until confirmed :-?
</BUGS>

TODO: When importing an ADIF file with several logs, create automatically the logs as detected.
TODO: HelpHelpDialog
TODO: HelpAboutDialog

TODO: setuppagelogs.cpp
TODO: Remove references to DataBase from all classes except DataProxySQLite

TODO: DXCluster: Lines that are not a DX should not be in another color than default.
TODO: Add a default DX Cluster server

TODO: Make a tool to mark and export QSO from the right button. (i.e. To mark several QSO to print and export the ADIF file with just those QSO)

TODO: Add all the Entity Info to the slotClear to clear everything.
TODO: Add a list of previous QSO with the same station, if any. (Done in the search box)

TODO: Create something like a void Awards::setAwardsOfAllQSO to read ALL QSO and set the Awards at once instead of adding one QSO per QSO


KLOG TODO:
TODO: To create a function tha runs the log and marks "N" if QSL has not been sent or received.
TODO: Create a setup page to configure a default prop_mode per band (ie 6m = ES)

TODO: CTY.DAT update
TODO: Award tabs: center/bold tabs
TODO: Add export to cabrillo to the logfile



SETUP:
TODO: Show progress when doing actions
TODO: Open this file when opening
TODO: DXCLuster: Show HF activity
TODO: DXCLuster: Show WARC
TODO: DXCLuster: Show VHUF
TODO: DXCLuster: Show confirmed
TODO: DXCLuster: Show SSB
TODO: DXCLuster: Show CW
TODO: DXCLuster: Show Ann/full
TODO: DXCLuster: Show WCY
TODO: DXCLuster: Show WWV
TODO: DXCLuster: Double click on a spot, add it to log
TODO: DXCLuster: Add Cluster servers
DONE: TODO: Colors: Confirmed, Worked, Needed band, New, Default

TODO: Require mandatory fields in all QSO

TODO: Awards: Add Award
TODO: Awards: Remove Award

=====================
<SATELLITE SUPPORT>
TODO: Sats: Create a way to update the list of supported satellites. Maybe another tab in the setup dialog as the World Editor
TODO: Sats: https://www.eqsl.cc/qslcard/ADIFContentSpecs.cfm
TODO: Sats: https://lotw.arrl.org/lotw/faq#sats

TODO: Sat Modes:
http://www.amsat.org/amsat/intro/sats_faq.html#RTFToC5
http://www.sckans.edu/~sireland/radio/amsat.html

A - This mode requires a 2 meter SSB/CW transmitter and a 10 meter SSB/CW receiver and supports CW and voice.
B - This mode requires a 70 cm SSB/CW transmitter and a 2 meter SSB/CW receiver and supports CW and voice. Some satellites also support RTTY and SSTV in this mode.
J -> V Uplink and U downlink
JA - This mode stands for J Analog and requires a 2 meter SSB/CW transmitter and a 70 cm SSB/CW receiver and supports CW, voice.
JD - This mode stands for J Digital and requires a 2 meter FM transmitter and a 70 cm SSB/CW receiver and supports packet.

K - This mode requires a 15 meter SSB/CW transmitter and a 10 meter SSB/CW receiver and supports CW and voice. This mode is unique in that it can be done with a simple HF rig.
S - This mode requires a 70 cm SSB/CW transmitter and a 2.4 GHz SSB/CW receiver and supports CW and voice. Many people use a 2.4 GHz to 2 meter converter with a 2 meter SSB/CW receiver instead of buying a 2.4 GHz SSB/CW receiver.
T - This mode requires a 15 meter SSB/CW transmitter and a 2 meter SSB/CW receiver and supports CW and voice.
KT, KA, BS, Some satellites have dual modes that operate simultaneously. For example, AO-13 can operate in mode BS which means that it can do both mode B and mode S simultaneously. Other common dual modes are KT and KA.

Mode V
Mode U
Mode U/V -> B
</SATELLITE SUPPORT>

TODO: Code a way to sort the bands/modes in the setuppagebandsmodes.cpp

TODO: Create an "updateKLog" class to manage all the release updates
so there is a way to detect the version of KLog and upgrade the DB to the latest.


TODO:
The following fields may add information, even if the qsl has not been rcvd/sent
<QSL_RCVD_VIA:1>B <QSL_SENT_VIA:1>B

TODO: showStatusOfDXCC should be executed when band change.

TODO: Add color support: messages for slotQRZTextChanged

TODO: SetupPageColors: Check the style in the buttons as the rounds are lost when I change the color!!

TODO: Check when to connect the DXCluster and when no, it tries twice or more...

TODO: Awards: make a function to calculate the total.

TODO: Color support: Add needed, worked, confirmed, neutral colors to the configuration dialog.
TODO: Color support: Support the bar when a QRZ is entered.
TODO: Color support: Calculate a color for the log.

TODO: World::getDXStatus: Calculate the algorithm to know the different status for a DXCC (confirmed, worked, confirmed in another band, ,...)
TODO: World:: Maybe the color should be returned from the World class

TODO: Check the readDataFromUI. QSO are not added when in contest.
TODO: Check that New Log, Open, ... somewhere the log table is removed from the DB!

TODO: The confirmed WAZ number is not properly calculated.

TODO: GUI: Add in the input box a combobox to change the CQZ
TODO: GUI: Add in the input box a combobox to change the ITUZ


TODO: In CQWWSSB, when editing QSO the SRX, Points, multiplier, ... are not sent to the edit so after "OK", those data are lost.

TODO: MainWindow::slotQsoDeleteFromLog: Add the CALL to the message before detele a QSO.

TODO: Search GUI: add multi-selection QSO to do the same actions inmultiple QSO.

TODO: When importing ADIF, update the logview sometimes... just to show the progress.
TODO: When importing ADIF: Only shows the ProgresDialog when the number is low >1000 <14000 investigate
TODO: Import Cabrillo


TODO: To check how can I order the columns in the log or in the search QTableView. Now the order depends only on the order of the SQL table.

TODO: When modifying a cell directly in the log, it is possible to select a mode/band that is not actually active in the configuration.

TODO: Slot: If (only)eqsl/lotw is sent/rec, the QSL_RCVD_VIA should be E

TODO: Code a Tool to get statistcs for the contests, some kind of post contest tool.
    http://www.qsl.net/3v4-002/Contests/2011%20CQ-WW-SSB%203V8SS/index.htm

TODO: Be able to send scores to: http://www.cqcontest.ru/help/developers.jsp

TODO: Create an update CTY.DAT without overwriting the current data. Just Adding and correcting (asking) if data is already there but different.
TODO: Create an export CTY.DAT file to create a CTY.DAT file with ALL the data in the current "world".



FILEMANAGER
TODO: adifLogExportToFile: Count the marked QSO and adjust the numberOfQsos
TODO: FileManager::adifReadLog: Optimize the dialog (maybe updating only each 100 or as in KLog)
TODO: FileManager::adifReadLog: Add a semaphore/lock or similar to avoid running the same method twice or more at the same time... or at least the same file.
        It seems that now it "serializes" the import...
TODO: Check that FileManager::adifLogExportToFile is exporting ALL the DB fields.
TODO: FileManager::adifLogExportToFile code a progress dialog for exporting.
TODO: When importing ADIF: Check if all the QSO have all the mandatory fields and warn the user if not.

Optimization: The ADIF import is very slow. Optimization is recommended.


IMPROVEMENT: Improve the result of the log printing.

DONE: TODO: Working on the DB version update functions
DONE: MainWindow::showAwards Remove "empty CQZ" when counting to avoid having 41 CQ zones
DONE: Code the color configuration for status of an entity (needed/worked/confirmed).
DONE: Color support: Calculate a color for the search results.
DONE: Color support: Calculate a color for the DXCluster.
DONE: TODO: Colors: Reconfigure the colors needs KLog to be restarted.
DONE: Working on the dxCluster: Color support, identify the different kind of lines... DX de, normal spots, comments, ...
DONE: Right click on log to show a to edit QSO.
DONE: Right click on log to show a QSL received.
DONE: Right click on log to remove a QSO.
DONE: Right click on log to show a QSL sent.
TODO: Right click on search to remove a QSO.
DONE: Right click on search to show a QSL reception.
DONE: Right click on search to show a QSL sent.
DONE: Right click on search to show to edit QSO.
DONE: Added a select/unselect all button to the search QSO tab.
DONE: Search QSO to send
DONE: Add a button to export to ADIF the content of searchResultsTreeWidget

DONE: When importing ADIF, if the CQZ/ITUZ/DXCC is empty, calculate and add it.
DONE: Not export ADIF fields if "N":
DONE: Print the log.
DONE: TODO: Time in UTC
DONE: TODO: Log in real time
DONE: Double click on cluster to select
DONE: TODO: When double clicking on a DX-Spot, frequency should be also copied to inputbox
DONE: TODO: When a DX-Spot is selected, the DX-Entity and status should be shown.
DONE: TODO: DXCluster: Connect, disconnect and connect again does not work
DONE: TODO: Add a field in Mainwindow to manage RX_PWR
DONE: TODO: slotclearbuttons->Colors to default
DONE: GUI: Add in the input box a combobox to change the DXCC
*/
