MSHV is a amateur radio software using the following modes
MSK For meteor scatter. Message frame duration is 72 ms and with Sh option 20 ms. Character transmission rate for standard messages is as high as 250 cps. JTMS For meteor scatter. Character transmission rate 197 cps. FSK441 For meteor scatter. Character transmission rate 147 cps. FSK315 For meteor scatter. Character transmission rate 105 cps. ISCAT Optimized for meteor and ionospheric scatter at 6 meters. Character transmission rate 16.15 or 32.3 cps. JT6M Optimized for meteor and ionospheric scatter at 6 meters. Character transmission rate 14.4 cps. FT4 Designed for HF contesting. FT8 Designed for fast tropospheric QSOs. JT65 VHF/UHF For EME and troposcatter. Q65 For ionospheric scatter, tropospheric scatter, rain scatter, TEP, and EME. PI4 PharusIgnis4 A digital modulation (MGM) for beacon purposes.
Developed by LZ2HV - Christo Tested by SP9HWY - Jurek and G0LFF - Dick Ideas about appearance OZ2M - Bo Linux binaries OZ1PIF - Peter, SK Linux and ARM binaries G8JVM - Richard Russian interface R5WM - Vladimir, SK Russian interface RU4NG - Igor Translations: Chinese Simplified and Traditional, VR2UPU - SZE-TO Wing Spanish and Catalan, EA3KE - Toni Olmo Portuguese, CU3AK - Jaime Eloy Romanian, YO3JW - Pit Stefan Fenyo Danish, 5P1KZX - Michael Polish, SP5QWB - Bartek French, ON6DP - Paul Brazilian Portuguese, PP7CJ - Crezivando Junior Norwegian, LA3QMA - Kai Gunter Brandt Italian, IW4ARD - Gianni Matteini Czech, OK1ABB - Miroslav Skoda Acknowledgements to K1JT Joe Taylor and WSJT Development Group. The algorithms, source code, look-and-feel of WSJT-X and related programs, and protocol specifications for the modes FSK441, FT8, JT4, JT6M, JT9, JT65, JTMS, QRA64, ISCAT, MSK144, are Copyright © 2001-2017 by one or more of the following authors: Joseph Taylor, K1JT; Bill Somerville, G4WJS; Steven Franke, K9AN; Nico Palermo, IV3NWV; Greg Beam, KI7MT; Michael Black, W9MDB; Edson Pereira, PY2SDR; Philip Karn, KA9Q; and other members of the WSJT Development Group. Acknowledgements to IU8LMC, Martino - ARI Caserta for FT2 mode.
MSHV is Open Source software licensed under the terms of Version 3 of the GNU General Public License (GPL) |
The project page for developers and source code can be found at https://sourceforge.net/projects/mshv/